**LIST OF SMS COMMANDS TO START GPS TRACKERS (TK103)**

Notes:

* In a command, **+** means you should concatenate the two elements besides the **+**
* **space** means you should put a space
* By default the password is **123456**
* Terms between **“”** should be written as they are

|  |  |  |
| --- | --- | --- |
| Command | Required | Description |
| “begin”+tracker\_password | Yes | To initialize the tracker |
| “password”+tracker\_password+space+new\_password | No | Change the tracker password  The password should not contain space |
| “GPRS”+tracker\_password | Yes | Set the GPRS mode to ON |
| “admin”+tracker\_password+space+phone\_number | Yes | Set an administrator for the Tracker  The maximum number of administrators is 5 (five)  The numbers defined are those which will receive alerts from the tracker |
| “time”+space+”zone”+ tracker\_password +space+tracker\_time\_zone | Yes | Set the time zone of the tracker  tracker\_time\_zone should be written with the sign (eg: +2, -3) |
| “APN”+tracker\_password+space+apn\_name | Yes | Define the APN of the GSM Network |
| “up”+tracker\_password+space+apn\_name+space+apn\_password | Yes | Define the parameters of APN |
| “adminip”+tracker\_password+space+ip\_address+space+”5001” | Yes | Define the IP Address of the Traccar Server |
| “fix010s0  00m\*\*\*n”+tracker\_password | Yes | Make the tracker send its location every 10 seconds |
| “distance”+tracker\_password+space+”0001” | Yes | Make the tracker send its location every 1 meter |
| “save010s\*\*\*n”+tracker\_password | Yes | Make the tracker store its locations in the SD Card when it loses the network signal |
| “angle”+tracker\_password+space+”001” | Yes | Make the tracker send its location every deviation of 1 degree |
| “suppress”+tracker\_password | Yes | Make the tracker stop sending its location when the engine in Off |